March 31, 2020

**CANADIAN TECHNICAL BULLETIN 002**

**TARGET MARKET ROOFING**

**Subject: Re-Roofing of roof assemblies containing Phenolic/Coal Tar Pitch**

In order to ensure the expected life cycle of Sika Sarnafil roof systems, Sika Sarnafil Canada requires all phenolic/Coal Tar Pitch materials to be removed prior to the installation of any new Materials when installing Sika Sarnafil related products.

In addition, all contaminated surfaces are to be cleaned in accordance with current Sika Sarnafil specification requirements. Where residue is still present after cleaning, effected surfaces must be covered with either plywood good one side or DensDeck Prime.

Please contact Sika Sarnafil Canada Roofing Technical Department for further information.