March 31, 2020

**CANADIAN TECHNICAL BULLETIN 008**

**TARGET MARKET ROOFING**

**Subject: Approved Welding Equipment for Sika Sarnafil Membranes**

This bulletin will define accepted seam welding equipment for use when welding Sika Sarnafil Canada membranes.

For automatic welders, all Sarnamatic series welders and Leister automatic welders approved for PVC field seam welding are accepted.

For hand welders, only the Liester hand welder series is accepted for use in welding our membranes.

All welding devices must be calibrated prior to use and welding must be done in accordance with accepted welding practices as instructed by Sika Sarnafil Canada Technical Department.

For further clarification or information regarding calibration of devices and best welding practices please contact Sika Sarnafil Canada Technical.